LDZX-30FBS 产品资料
上海申安LDZX-30FBS立式压力蒸汽灭菌器 高压灭菌锅消毒锅30L（停产）
本资料汇总当前产品页面的产品信息与技术资料，供选型与资料留存使用。
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产品状态：已停产
该型号已停产，以下产品介绍、技术参数与价格仅供历史资料查询。现售型号请参阅产品报价单或联系咨询。

	产品名称：翻盖式 不锈钢立式压力灭菌器

	型    号：LDZX-30FBS

	配    置：自动控制

	有效容积：30L

	外观特征： 全不锈钢

	功能简介：   

	◆自动控制灭菌循环程序

	◆时间任意设定（0-99小时）

	◆翻盖式结构

	◆超压自泄0.145-0.165Mpa

	◆灭菌终了蜂鸣器提醒后自动停机

	◆数码液晶窗显示工作状态

	◆温度任意设定（50℃-126℃）

	型     号     容积       电源       功率       灭菌室设计体积    重量       体积(mm)

	LDZX-30FBS 30L        220V      3KW       Φ350×330         65kg       560×590×980 
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产品页面 https://www.shshenan.cn/tingchan/LDZX-30FBS.html
product-1.png
RESmS

Medi

vy

o

N

al

hai

iy





product-2.jpg
e

A o A R B 2000 1) L o SRR TR
R—FAEFTFERRE R RHEREGKE . TRRE R HERI>
S H. 2Oy BB ARG AT R A T A S 45 BB X 69
WAOZHE, RESBUF. EiR. BE¥R, BERE. @0, L¥
RARERARNST. 1T, RERTFERLB—Y5ZHRHE.

AFAEM 201548 1 A 1 H-2020 4F 1 A 1 Hig4R.
5 b #8 #




product-3.jpg
) £ =REH

LDZX-30KBS

LDZX-50KBS

LDZX-75KBS
SRXENFERRER




product-4.jpg
LDZX-30FBS
LDZX-50FBS

SXENFERER




product-5.jpg
2. EREE

ARBTENEFRZEFR , FOERNENTRRITSHIENEXM
B, OADBTRAKFRIEIMEINES~RIEEFAIE , RE0EHT
i EEREEENRESANDET2NBHRE , £r2EHL
BEBREBM. MKERP. BREEENRERSKUNEER., FRIEE
RERAEHOHANBNCEZA , REEFTIRETHNEHEH ,
BREALINRREFERRENRADSNYEETHER , FREER
HREBERFFRAEEHTL  KBERANERERFARTE ,
REETRE. XERK. RRUT. EURNASRATEM. BH.
HR. BRBENL EFRESYRHTHSRENEES R,




product-6.jpg
£% /B8 Parameter /Model

R
Configuration

EFRHR

‘The main material

R/ £l
Volume/ GW

BB / T
Voltage / Power

BERY (K x 8 x # mm)

Packing sze. (Lx W x Hmm)

REESH (Hf2 x WA mm)

Sterilization chamber volume (diameter  height mm)

PIBE / R (I x FSEE mm )
Liner (diameter x height mm)/ Quanity

AR RS
‘Automatic control of the steriization cycle program
BRHYENRE

Interactive safety interlock device
BKERFIIRE

Water supply cut protecting equipment
BESERRE RS

Digital window display operating status
EJIERREEH

Time setting range.

|ETHEED

Maximum operating pressure
REREREE

Sterilzation temperature setting range

TRAUE —EBE S

Double scale numerical indication pressure gauge
BkES

Selfinfating type seal

RELEREDIRE

Sterilzation end automatic alarm.

LDZX-30KBS
LDZX-50KBS
LDZX-75KBS

)

Automatic control

TER

Stainless steel

30L/65Kg
50L/75Kg
75L/98Kg

220v/30Kw

220v/35 Kw
220735 Kw

560x590x980
560x590x1220
600x620x1410
350x330

350%520
388x650

FAE Basketx1/310x220
S Basketx2 /310x220
S Basketx3 /325x185.

Fiet
Hand Wheel

0990
0.165MPa

50-128°C

LDZX-30FBS
LDZX-50FBS

B

Automatic control

TR

Stainless steel

30L/65Kg
50L/75Kg

220V/30Kw
200735 Kw

560x590x980
560x590x1120

350%330
3504520

P Basketx1/310x220
FAE Basketx2 /310x220

|
Clamshell

0990
0165MPa

50-128°C




product-7.jpg
%

+4 4+ 3 3 3 3 33

FRER]

B ETBREFRUTE T8 (89 | PRIOGMERH 20000178 3)

B HHOEMEFTE 8 (89 : T52231005-2016)

B HATHE R W BATE

15090012008 BISKERMRIRNE" E#

R CEAE

RREWDN " LSETERERTR 1S

B LRBROETENTE %

SIS SRAREUREY

¥

+ 3+ 3 3

FRER

B —HFERTEBNE" ©F (THS $ 022654542)

B —EASEREGEREN TF (§18 : 2006200439791)

B EORESBORDSN T (FHS : 200020073672X )

T EASE (IE ) TR (GFS : 200630038964.1)

B RASURIKE G (TR : 2010201324236)

B TR (AR ) R (§HIS : 201030134837.8)

+4 3+ 3 33

FRAEN WS
BESTHRSEMTRSRANETIGIRE (ES | PRISKN (f ) 201392571466 8 )
SEEAIRES

B REE RSN BGEE (S : PRIOEN O ) 7 201382571708 8 )
BETRRETRSURNES B (S | PRIGEN Off) 720132570524 3)

BESTRREETRRSRNETEGEE (9 : PRIGEN () 7 2013 8 2571467 8 )




product-8.jpg
LML
4 e AR

K~ 2
WA, S
005 2 %

P (9

1 PEIRPNG VR 3T E )

1SO9001 Certifcationhich promises the relibity and sec &
m





